Follow import instructions below.
1-Unzip the Download

2-Copy/Paste the LEMANS SKP Files to your Insert Library Folder 

3-Import into the Insert Library within Mozaik
	-Go to the main title bar Libraries>Inserts 
	-Click your library you wish to import into 
	-Navigate to the unzipped location 
	-Import each .exp file 
	
4-The inserts are now uploaded to your library. Drag and drop them into your blind cabinets as required. 

5-Be mindful that the door has minimum door opening requirements below 

LeMans 40 - minimum opening is 14 1/4” (362 mm)
LeMans 45 - minimum opening is 16 1/2” (419 mm)
LeMans 50 - minimum opening is 18 3/8” (467 mm)
LeMans 60 - minimum opening is 22 1/4” (565 mm)

Consult the attached PDF for more info  

Always Cut one test cabinet from cover sheet to confirm drilling is coming out correct
